

Jason Schlottman


HWRS 582

**Streams\_Correct Figures**


**Initial figures produced:**









**Below are the plots produced with the same code, except the recharge rate was changed from 5E5 m/d to 1E5 m/d.**







**Finally the recharge rates were returned to initial conditions, but the bottom hydraulic conductivity "k\_strbott" was changed from 1 to 10 f/d**



